.\"                                      Hey, EMACS: -*- nroff -*-
.\" First parameter, NAME, should be all caps
.\" Second parameter, SECTION, should be 1-8, maybe w/ subsection
.\" other parameters are allowed: see man(7), man(1)
.TH RIGCTL "1" "December 03, 2003" "Hamlib"
.\" Please adjust this date whenever revising the manpage.
.\"
.\" Some roff macros, for reference:
.\" .nh        disable hyphenation
.\" .hy        enable hyphenation
.\" .ad l      left justify
.\" .ad b      justify to both left and right margins
.\" .nf        disable filling
.\" .fi        enable filling
.\" .br        insert line break
.\" .sp <n>    insert n+1 empty lines
.\" for manpage-specific macros, see man(7)
.SH NAME
rigmem \- backup and restore memory of radio transceivers and receivers
.SH SYNOPSIS
.B rigmem
[\fIOPTION\fR]... [\fICOMMAND\fR]...
.SH DESCRIPTION
Backup and restore memory of radio transceivers and receivers.
\fBrigmem\fP accepts \fBcommands\fP from command line only.
.PP
.\" TeX users may be more comfortable with the \fB<whatever>\fP and
.\" \fI<whatever>\fP escape sequences to invode bold face and italics, 
.\" respectively.
Keep in mind that \fBHamlib\fP is still BETA level software. 
A lof of stuff hasn't been tested thoroughly, and the API may change
without publicised notice. Please report bugs and feedback at
the e-mail address given in the REPORTING BUGS section.
.SH OPTIONS
This program follow the usual GNU command line syntax, with long
options starting with two dashes (`-').
A summary of options is included below.
.TP
.B \-m, \-\-model=id
Select radio model number. See model list, as reported by rigctl.
.TP
.B \-r, --rig-file=device
Use \fBdevice\fP as the file name of the radio to operate on.
.TP
.B \-s, --serial-speed=baud
Set serial speed to \fBbaud\fP rate. Uses maximal rig speed as default.
.TP
.B \-c, --civaddr=id
Use \fBid\fP as the CI-V address to communicate with the rig. 
Only for Icom rigs. NB: the id is in decimal, unless prefixed by \fB0x\fP,
in which case it is hexadecimal.
.TP
.B \-C, \-\-set\-conf=parm=val[,parm=val]*
Set config parameter.
.TP
.B \-x, \-\-xml
Use XML format instead of CSV, if libxml2 is available.
.TP
.B \-v, \-\-verbose
Set verbose mode, cumulative (BUG, ERR, WARN, VERBOSE, TRACE).
.TP
.B \-h, \-\-help
Show summary of options and exit.
.TP
.B \-V, \-\-version
Show version of program and exit.

.SH COMMANDS
Backup and restore are supported for basic CSV file and XML format where available.
.PP
Please note that the backend for the radio to be controlled, 
or the radio itself may not support some commands. In that case, 
the operation will fail with a standard error message.
.PP
A summary of commands is included below.
.TP
.B save
Save all the content of memory in a CSV (or XML) file given as argument to the command.
.TP
.B load
Load the content into all the memory from a CSV (or XML) file given as argument to the command.

.TP
.B save_parm
Save all the parameters of the radio in a CSV (or XML) file given as argument to the command.
.TP
.B load_parm
Load the parameters of the radio from a CSV (or XML) file given as argument to the command.

.TP
.B clear
Very DANGEROUS command, as it will completly clear out everything you have programmed 
in the memory of you radio. ALL DATA WILL BE LOST. Use at your own risks!

.SH RETURN VALUE
rigmem exits with:
0 if all operations went fine; 1 if there was an invalid command line
option or arg; or 2 if an error was returned by Hamlib.

.SH AUTHOR
Man page written by Stephane Fillod.
.SH BUGS
This almost empty section...
.SH REPORTING BUGS
Report bugs to <hamlib-developer@users.sourceforge.net>.
.br
I'm already aware of the bug in the previous section :-)
.SH COPYRIGHT
Copyright \(co 2000-2003 Stephane Fillod.
.br
This is free software; see the source for copying conditions.
There is NO warranty; not even for MERCHANTABILITY
or FITNESS FOR A PARTICULAR PURPOSE.
.SH SEE ALSO
.BR hamlib (3), rigctl(1)

