
You will find in the tests/ subdirectory various programs to exercise
the Hamlib library.
Most of the time, you will have to make sure that the backend for
your rig is loaded by passing the model number of your rig by argument.
If you don't know the number, listrigs can give it to you,
"rigctl --list" will also output something like this:

	Rig#	Mfg           Model           Vers.
	1		Hamlib        Dummy           0.1
	1506	Winradio      WR-3500         0.6
	210		Kenwood       TS-870S         0.1
	311		Icom          IC-706MkIIG     0.2
	105		Yaesu         FT-747GX        0.1
	[etc.]

In any case, you are encouraged to checked for correct initialization
by reading the source code, at the begining of the main(). Check also 
that the program is setup for your rig path strncpy(my_rig->state.rig_path...

dumpcaps  -	Output the caps contents of a rig 
dumpmem   -	Dump the memory contents of the rig 
listrigs  -	Condensed list of all the models supported by backends
rigmatrix -	Output the HTML table of supported rigs, with .png files for freqs
testbcd   -	Simple program to test BCD conversion, takes a number as arg.
testfreq  -	Simple program to test Freq conversion, takes a number as arg.
testrig   -	Sample program calling common API calls, uses rig_probe
testtrn   -	Sample program using event notification (transceive mode)
rigctl	  -	Combined tool to execute any call of the API, see man page
rigmem	  -	Combined tool to load/save content of rig memory, see man page

