____doifc
___boot_delay128k
___boot_delay12k
___boot_delay16k
___boot_delay24k
___boot_delay32k
___boot_delay48k
___boot_delay4k
___boot_delay64k
___boot_delay8k
__ca2aw
__cc2d
__cc2dw
__cca2aw
__ccs2s
__cs2s
__flash_size
__fzins
__low_savebsr
__low_savestatus
__low_savewreg
_adc_external_ref
_adc_external_vrefh
_adc_external_vrefl
_adc_internal_ref
a
abden
abden_bit
abdovf
abdovf_bit
access
ackdt
ackdt_bit
acken
acken_bit
ackstat
ackstat_bit
acqt0
acqt0_bit
acqt1
acqt1_bit
acqt2
acqt2_bit
acss
acss_bit
adc_get_sample
adc_get_sample_ptr
adc_init
adc_init_advanced
adc_read
adcon0
adcon1
adcon2
adcs0
adcs0_bit
adcs1
adcs1_bit
adcs2
adcs2_bit
add_32x32_fp
adden
adden_bit
aden
aden_bit
adfm
adfm_bit
adie
adie_bit
adif
adif_bit
adip
adip_bit
admsk1
admsk1_bit
admsk2
admsk2_bit
admsk3
admsk3_bit
admsk4
admsk4_bit
admsk5
admsk5_bit
adon
adon_bit
adres
adresh
adresl
an0
an0_bit
an1
an1_bit
an10
an10_bit
an11
an11_bit
an12
an12_bit
an2
an2_bit
an3
an3_bit
an4
an4_bit
an8
an8_bit
an9
an9_bit
atu_reset
auto
auto_delta
auto_mem
b0
b1
b2
b3
b4
b5
b6
b7
banked
baudcon
baudctl
bcd2dec
bcd2dec16
bclie
bclie_bit
bclif
bclif_bit
bclip
bclip_bit
bf
bf_bit
bgst
bgst_bit
bor
bor_bit
brg16
brg16_bit
brgh
brgh_bit
bsr
btn_push
but
button
button_delay
button_proc
button_proc_test
bypas
byte2double
bytetohex
bytetostr
bytetostrwithzeros
c
c_bit
c1inv
c1inv_bit
c1out_cmcon
c1out_cmcon_bit
c1out_porta
c1out_porta_bit
c2inv
c2inv_bit
c2out_cmcon
c2out_cmcon_bit
c2out_porta
c2out_porta_bit
cap_10
cap_100
cap_1000
cap_22
cap_220
cap_47
cap_470
cap_mem
cap_sw
cap1
cap2
cap3
cap4
cap5
cap6
cap7
ccp1
ccp1_bit
ccp1con
ccp1ie
ccp1ie_bit
ccp1if
ccp1if_bit
ccp1ip
ccp1ip_bit
ccp1m0
ccp1m0_bit
ccp1m1
ccp1m1_bit
ccp1m2
ccp1m2_bit
ccp1m3
ccp1m3_bit
ccp1x
ccp1x_bit
ccp1y
ccp1y_bit
ccp2_portb
ccp2_portb_bit
ccp2_portc
ccp2_portc_bit
ccp2con
ccp2ie
ccp2ie_bit
ccp2if
ccp2if_bit
ccp2ip
ccp2ip_bit
ccp2m0
ccp2m0_bit
ccp2m1
ccp2m1_bit
ccp2m2
ccp2m2_bit
ccp2m3
ccp2m3_bit
ccp2x
ccp2x_bit
ccp2y
ccp2y_bit
ccpr1
ccpr1h
ccpr1l
ccpr2
ccpr2h
ccpr2l
cells_init
cfgs
cfgs_bit
chs0
chs0_bit
chs1
chs1_bit
chs2
chs2_bit
chs3
chs3_bit
cis
cis_bit
ck
ck_bit
cke
cke_bit
ckp
ckp_bit
clki
clki_bit
clko
clko_bit
cm0
cm0_bit
cm1
cm1_bit
cm2
cm2_bit
cmcon
cmie
cmie_bit
cmif
cmif_bit
cmip
cmip_bit
coarse_cap
coarse_tune
comfrem
compare_double
correction
cren
cren_bit
csrc
csrc_bit
cvr0
cvr0_bit
cvr1
cvr1_bit
cvr2
cvr2_bit
cvr3
cvr3_bit
cvrcon
cvref
cvref_bit
cvren
cvren_bit
cvroe
cvroe_bit
cvrr
cvrr_bit
cvrss
cvrss_bit
d
d_a
d_a_bit
d_bit
d_not_a
d_not_a_bit
dc
dc_bit
dc1b0
dc1b0_bit
dc1b1
dc1b1_bit
dc2b0
dc2b0_bit
dc2b1
dc2b1_bit
dec2bcd
dec2bcd16
delay_100ms
delay_10ms
delay_10us
delay_1ms
delay_1sec
delay_1us
delay_22us
delay_500us
delay_50us
delay_5500us
delay_5ms
delay_80us
delay_8ms
delay_cyc
div_16x16_s
div_16x16_s_l
div_16x16_u
div_32x32_fp
div_32x32_s
div_32x32_u
div_8x8_s
div_8x8_u
done
done_bit
double2byte
double2int
double2longint
double2longword
double2word
dysp_cnt
dysp_cnt_mult
dysp_delay
dysp_off
dysp_on
eccp1as
eccp1del
eccpas
eccpas0
eccpas0_bit
eccpas1
eccpas1_bit
eccpas2
eccpas2_bit
eccpase
eccpase_bit
eeadr
eecon1
eecon2
eedata
eeie
eeie_bit
eeif
eeif_bit
eeip
eeip_bit
eepgd
eepgd_bit
eeprom_read
eeprom_write
equals_double
f
fast
ferr
ferr_bit
fid_loss
fixsign32
floattostr
floattostr_fixlen
flt0
flt0_bit
flts
flts_bit
forward
free
free_bit
fsr0
fsr0h
fsr0l
fsr0ptr
fsr1
fsr1h
fsr1l
fsr1ptr
fsr2
fsr2h
fsr2l
fsr2ptr
gcen
gcen_bit
get_forward
get_fosc_khz
get_pwr
get_reverse
get_swr
gie
gie_bit
gie_gieh
gie_gieh_bit
gieh
gieh_bit
giel
giel_bit
go
go_bit
go_done
go_done_bit
go_not_done
go_not_done_bit
hlvdcon
hlvden
hlvden_bit
hlvdie
hlvdie_bit
hlvdif
hlvdif_bit
hlvdin
hlvdin_bit
hlvdip
hlvdip_bit
hlvdl0
hlvdl0_bit
hlvdl1
hlvdl1_bit
hlvdl2
hlvdl2_bit
hlvdl3
hlvdl3_bit
ics_auto
ics_off
idlen
idlen_bit
ind_005
ind_011
ind_022
ind_045
ind_1
ind_22
ind_45
ind_mem
ind1
ind2
ind3
ind4
ind5
ind6
ind7
indf0
indf1
indf2
int0
int0_bit
int0e
int0e_bit
int0f
int0f_bit
int0ie
int0ie_bit
int0if
int0if_bit
int1
int1_bit
int1e
int1e_bit
int1f
int1f_bit
int1ie
int1ie_bit
int1if
int1if_bit
int1ip
int1ip_bit
int1p
int1p_bit
int2
int2_bit
int2double
int2e
int2e_bit
int2f
int2f_bit
int2ie
int2ie_bit
int2if
int2if_bit
int2ip
int2ip_bit
int2p
int2p_bit
intcon
intcon2
intcon3
intedg0
intedg0_bit
intedg1
intedg1_bit
intedg2
intedg2_bit
intsrc
intsrc_bit
inttohex
inttostr
inttostrwithzeros
iofs
iofs_bit
ipen
ipen_bit
ipr1
ipr2
ircf0
ircf0_bit
ircf1
ircf1_bit
ircf2
ircf2_bit
irvst
irvst_bit
ivrst
ivrst_bit
kbi0
kbi0_bit
kbi1
kbi1_bit
kbi2
kbi2_bit
kbi3
kbi3_bit
l
lata
lata0
lata0_bit
lata1
lata1_bit
lata2
lata2_bit
lata3
lata3_bit
lata4
lata4_bit
lata5
lata5_bit
lata6
lata6_bit
lata7
lata7_bit
latb
latb0
latb0_bit
latb1
latb1_bit
latb2
latb2_bit
latb3
latb3_bit
latb4
latb4_bit
latb5
latb5_bit
latb6
latb6_bit
latb7
latb7_bit
latc
latc0
latc0_bit
latc1
latc1_bit
latc2
latc2_bit
latc3
latc3_bit
latc4
latc4_bit
latc5
latc5_bit
latc6
latc6_bit
latc7
latc7_bit
lcd_ind
lcd_prep
lcd_prep_short
lcd_pwr
lcd_swr
led_init
led_send
led_wr_str
longint2double
longinttohex
longinttostrwithzeros
longjmp
longtostr
longword2double
longwordtohex
longwordtostr
longwordtostrwithzeros
loss_mode
ltrim
lvdcon
lvden
lvden_bit
lvdie
lvdie_bit
lvdif
lvdif_bit
lvdin
lvdin_bit
lvdip
lvdip_bit
lvdl0
lvdl0_bit
lvdl1
lvdl1_bit
lvdl2
lvdl2_bit
lvdl3
lvdl3_bit
lvv0
lvv0_bit
lvv1
lvv1_bit
lvv2
lvv2_bit
lvv3
lvv3_bit
main
mclr
mclr_bit
mul_16x16_s
mul_16x16_u
mul_32x32_fp
mul_32x32_s
mul_32x32_u
mul_8x8_s
n
n_bit
n_tx
not_a
not_a_bit
not_address
not_address_bit
not_bor
not_bor_bit
not_done
not_done_bit
not_mclr
not_mclr_bit
not_pd
not_pd_bit
not_por
not_por_bit
not_rbpu
not_rbpu_bit
not_ri
not_ri_bit
not_ss
not_ss_bit
not_t1sync
not_t1sync_bit
not_t3sync
not_t3sync_bit
not_to
not_to_bit
not_w
not_w_bit
not_write
not_write_bit
nrm3232
nrm4032
oerr
oerr_bit
oled_init
oled_wr_str
osc1
osc1_bit
osc2
osc2_bit
osccon
oscfie
oscfie_bit
oscfif
oscfif_bit
oscfip
oscfip_bit
osctune
osts
osts_bit
ov
ov_bit
p
p_bit
p_cnt
p_max
p_tx
pc
pcfg0
pcfg0_bit
pcfg1
pcfg1_bit
pcfg2
pcfg2_bit
pcfg3
pcfg3_bit
pcl
pclath
pclatu
pcu0
pcu0_bit
pcu1
pcu1_bit
pcu2
pcu2_bit
pcu3
pcu3_bit
pcu4
pcu4_bit
pd
pd_bit
peie
peie_bit
peie_giel
peie_giel_bit
pen
pen_bit
pgc
pgc_bit
pgd
pgd_bit
pgm
pgm_bit
pic_init
pie1
pie2
pir1
pir2
pllen
pllen_bit
plusw0
plusw1
plusw2
por
por_bit
port_to_tris_offset
porta
portb
portc
porte
postdec0
postdec1
postdec2
postinc0
postinc1
postinc2
power
power_old
pr2
preinc0
preinc1
preinc2
prod
prodh
prodl
prsen
prsen_bit
psa
psa_bit
pssac0
pssac0_bit
pssac1
pssac1_bit
pwm1con
pwr
r
r_bit
r_not_w
r_not_w_bit
r_w
r_w_bit
r0
r1
r10
r11
r12
r13
r14
r15
r16
r17
r18
r19
r2
r20
r3
r4
r5
r6
r7
r8
r9
ra0
ra0_bit
ra1
ra1_bit
ra2
ra2_bit
ra3
ra3_bit
ra4
ra4_bit
ra5
ra5_bit
ra6
ra6_bit
ra7
ra7_bit
rb0
rb0_bit
rb1
rb1_bit
rb2
rb2_bit
rb3
rb3_bit
rb4
rb4_bit
rb5
rb5_bit
rb6
rb6_bit
rb7
rb7_bit
rbie
rbie_bit
rbif
rbif_bit
rbip
rbip_bit
rbpu
rbpu_bit
rc0
rc0_bit
rc1
rc1_bit
rc2
rc2_bit
rc3
rc3_bit
rc4
rc4_bit
rc5
rc5_bit
rc6
rc6_bit
rc7
rc7_bit
rcen
rcen_bit
rcidl
rcidl_bit
rcie
rcie_bit
rcif
rcif_bit
rcip
rcip_bit
rcmt
rcmt_bit
rcon
rcreg
rcsta
rd
rd_bit
rd16
rd16_bit
rd16_t1con_bit
re3
re3_bit
res032
restart
ri
ri_bit
rready
rsen
rsen_bit
rtrim
rx_
rx__bit
rx9
rx9_bit
rx9d
rx9d_bit
rxdtp
rxdtp_bit
s
s_bit
sboren
sboren_bit
sck
sck_bit
sckp
sckp_bit
scl
scl_bit
scs0
scs0_bit
scs1
scs1_bit
sda
sda_bit
sdi
sdi_bit
sdiv3232l
sdo
sdo_bit
sen
sen_bit
send_command
sendb
sendb_bit
set_addressing
set_cap
set_ind
set_sw
setfdz32
setfov32
setfun32
setiov3224
setjmp
sharp_cap
sharp_ind
shorttohex
shorttostr
shorttostrwithzeros
show_loss
show_pwr
show_reset
smp
smp_bit
soft_i2c_init
soft_i2c_scl
soft_i2c_scl
soft_i2c_scl_direction
soft_i2c_scl_direction
soft_i2c_sda
soft_i2c_sda
soft_i2c_sda_direction
soft_i2c_sda_direction
soft_i2c_start
soft_i2c_stop
soft_i2c_write
soft_tune
sp0
sp0_bit
sp1
sp1_bit
sp2
sp2_bit
sp3
sp3_bit
sp4
sp4_bit
spbrg
spbrgh
spen
spen_bit
sren
sren_bit
ss
ss_bit
sspadd
sspbuf
sspcon1
sspcon2
sspen
sspen_bit
sspie
sspie_bit
sspif
sspif_bit
sspip
sspip_bit
sspm0
sspm0_bit
sspm1
sspm1_bit
sspm2
sspm2_bit
sspm3
sspm3_bit
sspov
sspov_bit
sspstat
status
stkful
stkful_bit
stkovf
stkovf_bit
stkptr
stkunf
stkunf_bit
sub_32x32_fp
sub_tune
sw_mem
swap
swdte
swdte_bit
swdten
swdten_bit
swr
swr_a
swr_fixed_old
swr_old
sync
sync_bit
t016bit
t016bit_bit
t08bit
t08bit_bit
t0cki
t0cki_bit
t0con
t0cs
t0cs_bit
t0ie
t0ie_bit
t0if
t0if_bit
t0ps0
t0ps0_bit
t0ps1
t0ps1_bit
t0ps2
t0ps2_bit
t0ps3
t0ps3_bit
t0se
t0se_bit
t13cki
t13cki_bit
t1cki
t1cki_bit
t1ckps0
t1ckps0_bit
t1ckps1
t1ckps1_bit
t1con
t1oscen
t1oscen_bit
t1osi
t1osi_bit
t1oso
t1oso_bit
t1run
t1run_bit
t1sync
t1sync_bit
t2ckps0
t2ckps0_bit
t2ckps1
t2ckps1_bit
t2con
t2outps0
t2outps0_bit
t2outps1
t2outps1_bit
t2outps2
t2outps2_bit
t2outps3
t2outps3_bit
t3ccp1
t3ccp1_bit
t3ccp2
t3ccp2_bit
t3ckps0
t3ckps0_bit
t3ckps1
t3ckps1_bit
t3con
t3sync
t3sync_bit
tablat
tblptr
tblptrh
tblptrl
tblptru
tblptru0
tblptru0_bit
tblptru1
tblptru1_bit
tblptru2
tblptru2_bit
tblptru3
tblptru3_bit
tblptru4
tblptru4_bit
test
test_init
tmr0h
tmr0ie
tmr0ie_bit
tmr0if
tmr0if_bit
tmr0ip
tmr0ip_bit
tmr0l
tmr0on
tmr0on_bit
tmr1cs
tmr1cs_bit
tmr1h
tmr1ie
tmr1ie_bit
tmr1if
tmr1if_bit
tmr1ip
tmr1ip_bit
tmr1l
tmr1on
tmr1on_bit
tmr2
tmr2ie
tmr2ie_bit
tmr2if
tmr2if_bit
tmr2ip
tmr2ip_bit
tmr2on
tmr2on_bit
tmr3cs
tmr3cs_bit
tmr3h
tmr3ie
tmr3ie_bit
tmr3if
tmr3if_bit
tmr3ip
tmr3ip_bit
tmr3l
tmr3on
tmr3on_bit
to_
to__bit
tosh
tosl
tosu
toutps0
toutps0_bit
toutps1
toutps1_bit
toutps2
toutps2_bit
toutps3
toutps3_bit
track
trisa
trisa0
trisa0_bit
trisa1
trisa1_bit
trisa2
trisa2_bit
trisa3
trisa3_bit
trisa4
trisa4_bit
trisa5
trisa5_bit
trisa6
trisa6_bit
trisa7
trisa7_bit
trisb
trisb0
trisb0_bit
trisb1
trisb1_bit
trisb2
trisb2_bit
trisb3
trisb3_bit
trisb4
trisb4_bit
trisb5
trisb5_bit
trisb6
trisb6_bit
trisb7
trisb7_bit
trisc
trisc0
trisc0_bit
trisc1
trisc1_bit
trisc2
trisc2_bit
trisc3
trisc3_bit
trisc4
trisc4_bit
trisc5
trisc5_bit
trisc6
trisc6_bit
trisc7
trisc7_bit
trmt
trmt_bit
tun0
tun0_bit
tun1
tun1_bit
tun2
tun2_bit
tun3
tun3_bit
tun4
tun4_bit
tune
tx
tx_bit
tx9
tx9_bit
tx9d
tx9d_bit
txckp
txckp_bit
txen
txen_bit
txie
txie_bit
txif
txif_bit
txip
txip_bit
txreg
txsta
type
ua
ua_bit
vcfg0
vcfg0_bit
vcfg1
vcfg1_bit
vdelay_advanced_ms
vdelay_ms
vdirmag
vdirmag_bit
vpp
vpp_bit
vref_mask
vrefn
vrefn_bit
vrefp
vrefp_bit
w
wcol
wcol_bit
wdtcon
word2double
wordtohex
wordtostr
wordtostrwithzeros
work_char
work_int
work_str
work_str_2
wr
wr_bit
wreg
wren
wren_bit
wrerr
wrerr_bit
wue
wue_bit
z
z_bit
