(kicad_pcb (version 20171130) (host pcbnew 5.1.5-1.fc31)

  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 0)
    (zones 0)
    (modules 0)
    (nets 1)
  )

  (page USLetter)
  (title_block
    (title "NucleoTNC Spacer")
    (date 2020-05-05)
    (rev B)
    (company "Mobilinkd TNC")
    (comment 1 "1.6mm FR4")
  )

  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x210e0_7ffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (dimension 21.001488 (width 0.15) (layer Dwgs.User)
    (gr_text "21.001 mm" (at 160.625508 96.417645 0.6820603932) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 171 85.75) (xy 171.117013 95.579116)))
    (feature2 (pts (xy 150 86) (xy 150.117013 95.829116)))
    (crossbar (pts (xy 150.110033 95.242737) (xy 171.110033 94.992737)))
    (arrow1a (pts (xy 171.110033 94.992737) (xy 169.99059 95.592526)))
    (arrow1b (pts (xy 171.110033 94.992737) (xy 169.976628 94.419768)))
    (arrow2a (pts (xy 150.110033 95.242737) (xy 151.243438 95.815706)))
    (arrow2b (pts (xy 150.110033 95.242737) (xy 151.229476 94.642948)))
  )
  (gr_text "Please place Production Code here on front silkscreen." (at 164 81.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_line (start 164 82.5) (end 165.25 82.5) (layer F.Fab) (width 0.15))
  (gr_line (start 161.5 84.5) (end 164 82.5) (layer F.Fab) (width 0.15))
  (gr_circle (center 161 84.75) (end 161 85.25) (layer F.Fab) (width 0.15))
  (dimension 18 (width 0.15) (layer Dwgs.User)
    (gr_text "18.000 mm" (at 160.5 92.05) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 151.5 86) (xy 151.5 91.336421)))
    (feature2 (pts (xy 169.5 86) (xy 169.5 91.336421)))
    (crossbar (pts (xy 169.5 90.75) (xy 151.5 90.75)))
    (arrow1a (pts (xy 151.5 90.75) (xy 152.626504 90.163579)))
    (arrow1b (pts (xy 151.5 90.75) (xy 152.626504 91.336421)))
    (arrow2a (pts (xy 169.5 90.75) (xy 168.373496 90.163579)))
    (arrow2b (pts (xy 169.5 90.75) (xy 168.373496 91.336421)))
  )
  (gr_arc (start 169 86) (end 169 86.5) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 152 86) (end 152 85.5) (angle -180) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152 86.5) (end 169 86.5) (layer Edge.Cuts) (width 0.05) (tstamp 5EB21275))
  (gr_line (start 152 85.5) (end 169 85.5) (layer Edge.Cuts) (width 0.05))
  (dimension 4 (width 0.12) (layer Dwgs.User) (tstamp 5EB211EA)
    (gr_text "4.000 mm" (at 176.77 86 270) (layer Dwgs.User) (tstamp 5EB211EA)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 165.75 88) (xy 176.086421 88)))
    (feature2 (pts (xy 165.75 84) (xy 176.086421 84)))
    (crossbar (pts (xy 175.5 84) (xy 175.5 88)))
    (arrow1a (pts (xy 175.5 88) (xy 174.913579 86.873496)))
    (arrow1b (pts (xy 175.5 88) (xy 176.086421 86.873496)))
    (arrow2a (pts (xy 175.5 84) (xy 174.913579 85.126504)))
    (arrow2b (pts (xy 175.5 84) (xy 176.086421 85.126504)))
  )
  (gr_text SPACER (at 160.5 87.25) (layer F.SilkS)
    (effects (font (size 1 1.5) (thickness 0.1)))
  )
  (gr_arc (start 169 86) (end 169 88) (angle -90) (layer Edge.Cuts) (width 0.05) (tstamp 5EB211E6))
  (gr_arc (start 152 86) (end 150 86) (angle -90) (layer Edge.Cuts) (width 0.05) (tstamp 5EB211E0))
  (gr_arc (start 169 86) (end 171 86) (angle -90) (layer Edge.Cuts) (width 0.05) (tstamp 5EB211EF))
  (gr_arc (start 152 86) (end 152 84) (angle -90) (layer Edge.Cuts) (width 0.05) (tstamp 5EB211F2))
  (gr_line (start 152 88) (end 169 88) (layer Edge.Cuts) (width 0.05) (tstamp 5EB211F5))
  (gr_line (start 152 84) (end 169 84) (layer Edge.Cuts) (width 0.05) (tstamp 5EB211E3))

)
