[![stratux version](https://img.shields.io/github/tag/cyoung/stratux.svg?style=flat&label=stratux)](https://github.com/cyoung/stratux/releases)
[![Build Status](http://circleci-badges-max.herokuapp.com/img/cyoung/stratux/master?token=:circle-ci-token)](https://circleci.com/gh/cyoung/stratux/tree/master)
[![BSD3 License](http://img.shields.io/badge/license-BSD3-brightgreen.svg)](https://tldrlegal.com/license/bsd-3-clause-license-%28revised%29)
# stratux
RTL-SDR UAT tools


Use Pi 2 and ForeFlight 7.3.1 (1792) (Sep 18, 2015).


Supported WiFi adapters:
* Edimax EW-7811Un

Tested RTL-SDR:
* NooElec NESDR Nano 2 (best)
* NooElec NESDR Mini 2
* Generic R820T (degraded performance)

Apps with stratux recognition/support:
* Seattle Avionics FlyQ EFB 2.1.1+.
* AvNav EFB 2.0.0+.
* Naviator.
* WingX Pro7 8.6.2+
* FltPlan Go.

Tested weather/traffic displays:
* ForeFlight 7+ - weather, traffic, AHRS.
* Avare
* iFly 740 - weather & traffic.


https://www.reddit.com/r/stratux
