# This file was automatically created based on description files (*.desc)
# by sane-desc 3.5 from sane-backends 1.0.24git on Thu Aug  1 18:50:15 2013
#
# udev rules file for supported USB and SCSI devices
#
# For the list of supported USB devices see /usr/lib/udev/hwdb.d/20-sane.hwdb
#
# The SCSI device support is very basic and includes only
# scanners that mark themselves as type "scanner" or
# SCSI-scanners from HP and other vendors that are entitled "processor"
# but are treated accordingly.
#
# If your SCSI scanner isn't listed below, you can add it to a new rules
# file under /etc/udev/rules.d/.
#
# If your scanner is supported by some external backend (brother, epkowa,
# hpaio, etc) please ask the author of the backend to provide proper
# device detection support for your OS
#
# If the scanner is supported by sane-backends, please mail the entry to
# the sane-devel mailing list (sane-devel@alioth-lists.debian.net).
#
ACTION!="add", GOTO="libsane_rules_end"

# The following rule will disable USB autosuspend for the device
ENV{DEVTYPE}=="usb_device", ENV{libsane_matched}=="yes", TEST=="power/control", ATTR{power/control}="on"

SUBSYSTEMS=="scsi", GOTO="libsane_scsi_rules_begin"
GOTO="libsane_rules_end"

LABEL="libsane_scsi_rules_begin"
KERNEL!="sg[0-9]*", GOTO="libsane_rules_end"

# Generic: SCSI device type 6 indicates a scanner
ATTRS{type}=="6", ENV{libsane_matched}="yes"

# Some scanners advertise themselves as SCSI device type 3

# Wildcard: for some Epson SCSI scanners
ATTRS{type}=="3", ATTRS{vendor}=="EPSON", ATTRS{model}=="SCANNER*", ENV{libsane_matched}="yes"

# Epson Perfection 2450 | Epson Perfection 2450 PHOTO
ATTRS{type}=="3", ATTRS{vendor}=="EPSON", ATTRS{model}=="GT-9700", ENV{libsane_matched}="yes"

# Epson Perfection 3200 | Epson Perfection 3200 PHOTO
ATTRS{type}=="3", ATTRS{vendor}=="EPSON", ATTRS{model}=="GT-9800", ENV{libsane_matched}="yes"

# Epson Perfection 636S | Epson Perfection 1200S
ATTRS{type}=="3", ATTRS{vendor}=="EPSON", ATTRS{model}=="Perfection1200", ENV{libsane_matched}="yes"

# Epson Perfection 636
ATTRS{type}=="3", ATTRS{vendor}=="EPSON", ATTRS{model}=="Perfection636", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet 4p
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C1130A", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet IIc
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C1750A", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet IIp
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C1790A", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet IIcx
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C2500A", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet 4c
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C2520A", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet 5p
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C5110A", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet 6200C
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C6270A", ENV{libsane_matched}="yes"

# Hewlett-Packard ScanJet 6300C
ATTRS{type}=="3", ATTRS{vendor}=="HP", ATTRS{model}=="C7670A", ENV{libsane_matched}="yes"


LABEL="libsane_rules_end"
